{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":253,"n_cols":5,"rows_kept":253,"merged":[[0,0,0,4],[2,1,2,2],[7,1,7,2],[28,1,28,2],[52,1,52,2],[65,1,65,2],[69,1,69,2],[77,1,79,1],[80,1,80,2],[81,1,81,2],[82,1,82,2],[84,1,85,1],[87,0,87,4],[89,1,89,2],[94,1,94,2],[115,1,115,2],[138,1,138,2],[151,1,151,2],[155,1,155,2],[163,1,165,1],[166,1,166,2],[167,1,167,2],[168,1,168,2],[170,1,171,1],[173,0,173,4],[204,0,204,4],[217,0,217,4],[230,0,230,4],[234,0,234,3],[238,0,238,4],[252,0,252,4]],"flags":["formulas_cached_only"]}
["一号温室（共计4跨，每跨7.2米，其中两跨长11开间44米，两跨长12开间48米，占地1324.8平方米）"]
["序号","名  称","品牌、规格型号","单位","总数量"]
["一","基 础 "]
[1.1,"钢筋预制件","φ14×2×100×450","套",62]
[1.2,"立柱基础","φ400*600mm","个",62]
[1.2999999999999998,"内部地面处理","素土夯实后铺设黑色园艺地布","㎡",1324.8]
[1.3999999999999997,"挡土墙","30cm高×24cm 宽，内外水泥砂浆抹平","米",149.6]
["二","主框架，配件 "]
[2.1,"端面主立柱","□80×60×3×4000 热镀锌","支",62]
[2.2,"端面立杆","□50×30×2×5300 热镀锌","支",16]
[2.3000000000000003,"端面立杆","□50×30×2×6600 热镀锌","支",16]
[2.4000000000000004,"横拉杆","□60×40×2×7118 热镀锌","支",50]
[2.5000000000000004,"侧副立柱","□50×30 热镀锌","支",23]
[2.6000000000000005,"新型辊压天沟","L=4000 δ=2.0mm 热镀锌","条",58]
[2.7000000000000006,"托架","热镀锌板冲压","只",62]
[2.8000000000000007,"水斗","热镀锌板冲压","只",10]
[2.900000000000001,"天沟加强板","2.5mm","只",174]
[{"v":2.1,"d":"2.10"},"主拱杆","φ50×25×1.5mm 四米一根","支",50]
[2.11,"副拱杆","φ32×1.5mm一米一根","支",276]
[{"v":2.1199999999999997,"d":"2.12"},"拉杆","φ32×1.5×6000","支",92]
[2.1299999999999994,"横拉杆吊杆","Φ32×1.5mm 热镀锌","支",42]
[{"v":2.1399999999999992,"d":"2.14"},"端面水平斜撑","Φ48×2","支",16]
[2.149999999999999,"斜拉筋","Φ12×4260","支",20]
[{"v":2.159999999999999,"d":"2.16"},"柱间支撑","□60×40×2×3900 热镀锌","支",20]
[2.1699999999999986,"卡槽","L=4000,0.7mm热镀锌板材","米",1152]
[{"v":2.1799999999999984,"d":"2.18"},"卡槽弹簧","L=2000  包塑","米",1152]
[2.189999999999998,"PVC 落水管","Φ110×4000","支",10]
[{"v":2.199999999999998,"d":"2.20"},"PVC 弯头","Φ110","只",10]
["三","外遮阳系统 "]
[3.1,"端面立柱","□50×50×2×2500 热镀锌","支",62]
[3.2,"立柱纵拉杆","□50×30×2×3948 热镀锌","支",58]
[3.3,"立柱横拉杆","□50×50×2×7148 热镀锌","支",50]
[3.4000000000000004,"水平斜撑","Φ48×2","支",16]
[3.5000000000000004,"立柱斜拉筋","Φ12×4005","支",20]
[3.6000000000000005,"传动轴平面支撑","Φ32×1.5×4500 热镀锌","支",8]
[3.7000000000000006,"减速电机","WJN-80","台",1]
[3.8000000000000007,"电机底板","热镀锌","块",1]
[3.900000000000001,"传动轴 1","Φ33×295×2.5","支",1]
[{"v":3.1,"d":"3.10"},"传动轴 2","Φ33×3225×2.5","支",1]
[3.11,"传动轴 3","Φ33×3175×2.5","支",1]
[{"v":3.1199999999999997,"d":"3.12"},"传动轴 4","Φ33×3875×2.5","支",5]
[{"v":3.1299999999999994,"d":"3.13"},"齿轮座，齿条","A 型","套",10]
[{"v":3.1399999999999992,"d":"3.14"},"驱动杆","Φ32×1.5×4050","支",80]
[{"v":3.149999999999999,"d":"3.15"},"驱动杆导座",null,"套",70]
[{"v":3.159999999999999,"d":"3.16"},"定位卡","单脚 Φ22","只",196]
[{"v":3.1699999999999986,"d":"3.17"},"定位卡","双脚 Φ22","只",420]
[{"v":3.1799999999999984,"d":"3.18"},"活动幕杆","Φ22×6000","支",57]
[{"v":3.189999999999998,"d":"3.19"},"托幕线","黑色 Φ2.3","米",1980]
[{"v":3.199999999999998,"d":"3.20"},"水平杆斜撑","Φ32×1.5×3025","支",100]
[{"v":3.2099999999999977,"d":"3.21"},"压膜卡","Φ22","只",684]
[{"v":3.2199999999999975,"d":"3.22"},"圆卡箍","Φ22","只",85.5]
[{"v":3.2299999999999973,"d":"3.23"},"黑色外遮阳网","遮阳率 75% 4.2m宽","㎡",1453.2]
["四","通风系统 "]
[4.1,"卷膜器","电动动顶开窗","套",6]
[4.2,"卷膜器","电动动侧开窗","套",4]
[4.300000000000001,"卷膜杆","Φ22×6000","米",283]
[4.400000000000001,"压膜卡","Φ22","只",424.5]
[4.500000000000002,"八字簧","包塑","只",192]
[4.600000000000002,"压膜绳","200m","米",1536]
[4.700000000000003,"爬行杆","φ25×1.2×3000","支",10]
[4.800000000000003,"伸缩杆","φ32×250","套",10]
[4.900000000000004,"棚门","2m×2m 热镀锌方管双开门","樘",1]
[{"v":4.1,"d":"4.10"},"门上轨","C 型铝合金 L=4000","支",1]
[4.11,"门下轨","∠4 角铁  L=4000","支",1]
[4.12,"门横梁","□40×60×2×4000 热镀锌","支",1]
["五","降温系统 "]
[5.1,"负压风机","1380 型","台",3]
[5.2,"湿帘","1.5m高，宽×0.1m 厚","㎡",39]
[5.3,"循环水管道","PVC 管材","套",1]
["六","覆盖系统 "]
[6.1,"棚顶膜","15 丝 PO ","㎡",1472]
[6.2,"端面膜","15 丝 PO ","㎡",345.6]
[6.300000000000001,"侧面膜","15 丝 PO ","㎡",394]
[6.400000000000001,"顶裙膜","15 丝 PO 0.6m","㎡",165.6]
[6.500000000000002,"侧裙膜","15 丝 PO 0.6m","㎡",55.2]
[6.600000000000002,"端裙膜","15 丝 PO 0.6m","㎡",55.2]
[6.700000000000003,"固定膜","15 丝 PO 1.2m","㎡",20]
[6.800000000000003,"防虫网","30 目  1m","㎡",316.8]
[6.900000000000004,null,"30 目  1.5m","㎡",158]
[{"v":6.1,"d":"6.10"},null,"30 目  1.5m","㎡",108]
["七","标准件 "]
[7.1,"螺栓、自钻钉、双面贴、钢丝固定卡、扎丝、挂网扣",null,"项",1]
["八","电路电线 "]
[8.1,"电路控制系统","电器电路主控制柜","套",2]
[8.2,"电线","3×1.5 ㎡ 风机线","米",136]
[8.3,null,"6×1 ㎡ 拉幕电机线","米",82]
["九","施工安装服务","包括温室全部施工安装","㎡",1324.8]
["二号温室（共计3跨，每跨7.2米，长度48米，每跨相对错开占地1036.8平方米）"]
["序号","名  称","品牌、规格型号","单位","总数量"]
["一","基 础 "]
[1.1,"钢筋预制件","φ14×2×100×450","套",52]
[1.2,"立柱基础","φ400*600mm","个",52]
[1.2999999999999998,"内部地面处理","素土夯实后铺设黑色园艺地布","㎡",1036.8]
[1.3999999999999997,"挡土墙","30cm高×24cm 宽，内外水泥砂浆抹平","米",139.2]
["二","主框架，配件 "]
[2.1,"端面主立柱","□80×60×3×4000 热镀锌","支",52]
[2.2,"端面立杆","□50×30×2×5300 热镀锌","支",12]
[2.3000000000000003,"端面立杆","□50×30×2×6600 热镀锌","支",12]
[2.4000000000000004,"横拉杆","□60×40×2×7118 热镀锌","支",39]
[2.5000000000000004,"侧副立柱","□50×30 热镀锌","支",24]
[2.6000000000000005,"新型辊压天沟","L=4000 δ=2.0mm 热镀锌","条",48]
[2.7000000000000006,"托架","热镀锌板冲压","只",52]
[2.8000000000000007,"水斗","热镀锌板冲压","只",8]
[2.900000000000001,"天沟加强板","2.5mm","只",144]
[{"v":2.1,"d":"2.10"},"主拱杆","φ50×25×1.5mm 四米一根","支",39]
[2.11,"副拱杆","φ32×1.5mm一米一根","支",216]
[{"v":2.1199999999999997,"d":"2.12"},"拉杆","φ32×1.5×6000","支",72]
[2.1299999999999994,"横拉杆吊杆","Φ32×1.5mm 热镀锌","支",33]
[{"v":2.1399999999999992,"d":"2.14"},"端面水平斜撑","Φ48×2","支",12]
[2.149999999999999,"斜拉筋","Φ12×4260","支",16]
[{"v":2.159999999999999,"d":"2.16"},"柱间支撑","□60×40×2×3900 热镀锌","支",16]
[2.1699999999999986,"卡槽","L=4000,0.7mm热镀锌板材","米",850]
[{"v":2.1799999999999984,"d":"2.18"},"卡槽弹簧","L=2000  包塑","米",850]
[2.189999999999998,"PVC 落水管","Φ110×4000","支",8]
[{"v":2.199999999999998,"d":"2.20"},"PVC 弯头","Φ110","只",8]
["三","外遮阳系统 "]
[3.1,"端面立柱","□50×50×2×2500 热镀锌","支",52]
[3.2,"立柱纵拉杆","□50×30×2×3948 热镀锌","支",48]
[3.3,"立柱横拉杆","□50×50×2×7148 热镀锌","支",39]
[3.4000000000000004,"水平斜撑","Φ48×2","支",12]
[3.5000000000000004,"立柱斜拉筋","Φ12×4005","支",16]
[3.6000000000000005,"减速电机","WJN-80","台",1]
[3.7000000000000006,"电机底板","热镀锌","块",1]
[3.8000000000000007,"传动轴 1","Φ33×295×2.5","支",1]
[3.900000000000001,"传动轴 2","Φ33×3225×2.5","支",1]
[{"v":3.1,"d":"3.10"},"传动轴 3","Φ33×3175×2.5","支",1]
[3.11,"传动轴 4","Φ33×3875×2.5","支",3]
[{"v":3.1199999999999997,"d":"3.12"},"齿轮座，齿条","A 型","套",8]
[{"v":3.1299999999999994,"d":"3.13"},"驱动杆","Φ32×1.5×4050","支",96]
[{"v":3.1399999999999992,"d":"3.14"},"驱动杆导座",null,"套",88]
[{"v":3.149999999999999,"d":"3.15"},"定位卡","单脚 Φ22","只",231]
[{"v":3.159999999999999,"d":"3.16"},"定位卡","双脚 Φ22","只",495]
[{"v":3.1699999999999986,"d":"3.17"},"活动幕杆","Φ22×6000","支",44]
[{"v":3.1799999999999984,"d":"3.18"},"托幕线","黑色 Φ2.3","米",2205]
[{"v":3.189999999999998,"d":"3.19"},"水平杆斜撑","Φ32×1.5×3025","支",78]
[{"v":3.199999999999998,"d":"3.20"},"压膜卡","Φ22","只",528]
[{"v":3.2099999999999977,"d":"3.21"},"圆卡箍","Φ22","只",66]
[{"v":3.2199999999999975,"d":"3.22"},"黑色外遮阳网","遮阳率 75% 4.2m宽","㎡",1159.2]
[{"v":3.2299999999999973,"d":"3.23"},"通风系统 "]
["四","卷膜器","电动动顶开窗","套",4]
[4.1,"卷膜器","电动动侧开窗","套",4]
[4.2,"卷膜杆","Φ22×6000","米",331]
[4.300000000000001,"压膜卡","Φ22","只",496.5]
[4.400000000000001,"八字簧","包塑","只",288]
[4.500000000000002,"压膜绳","200m","米",1713.6]
[4.600000000000002,"爬行杆","φ25×1.2×3000","支",8]
[4.700000000000003,"伸缩杆","φ32×250","套",8]
[4.800000000000003,"棚门","2m×2m 热镀锌方管双开门","樘",1]
[4.900000000000004,"门上轨","C 型铝合金 L=4000","支",1]
[{"v":4.1,"d":"4.10"},"门下轨","∠4 角铁  L=4000","支",1]
[4.11,"门横梁","□40×60×2×4000 热镀锌","支",1]
[4.12,"降温系统 "]
["五","负压风机","1380 型","台",2]
[5.1,"湿帘","1.5m 高×3.5m 宽×0.1m 厚","㎡",32]
[5.2,"循环水管道","PVC 管材","套",1]
[5.3,"覆盖系统 "]
["六","棚顶膜","15 丝 PO ","㎡",1152]
[6.1,"端面膜","15 丝 PO ","㎡",259.2]
[6.2,"侧面膜","15 丝 PO ","㎡",384]
[6.300000000000001,"顶裙膜","15 丝 PO 0.6m","㎡",115]
[6.400000000000001,"侧裙膜","15 丝 PO 0.6m","㎡",57.6]
[6.500000000000002,"端裙膜","15 丝 PO 0.6m","㎡",26]
[6.600000000000002,"固定膜","15 丝 PO 1.2m","㎡",16]
[6.700000000000003,"防虫网","30 目  1m","㎡",230]
[6.800000000000003,null,"30 目  1.5m","㎡",172]
[6.900000000000004,null,"30 目  1.5m","㎡",70]
[{"v":6.1,"d":"6.10"},"标准件 "]
["七","螺栓、自钻钉、双面贴、钢丝固定卡、扎丝、挂网扣",null,"项",1]
[7.1,"电路电线 "]
["八","电路控制系统","电器电路主控制柜","套",2]
[8.1,"电线","3×1.5 ㎡ 风机线","米",102]
[8.2,null,"6×1 ㎡ 拉幕电机线","米",71.6]
[8.3,"施工安装服务","包括温室全部施工安装","㎡",1036.8]
["单体钢架大棚2130㎡跨度6米，定稿3米，肩高1.5米（垂直于地面）"]
["跨度（m）","顶高（m）","肩高（m）","拱间距（m）","侧倾角"]
[6,3,1.5,0.8,"80°"]
["序号","名称","规格型号","单位","数量"]
[1,"拱杆","热浸镀锌钢管，φ25*1.2mm","支",1414]
[2,"抗风斜撑","热浸镀锌钢管，φ25*1.2mm","支",28]
[3,"外棚纵拉杆","热浸镀锌钢管，φ25*1.2*6000mm","支",178]
[4,"拱杆连接管","热浸镀锌钢管，φ25*1.5m","只",707]
[5,"棚头立柱 l","热浸镀锌钢管，φ25*1.2*2800mm","支",14]
[6,"棚头立柱 2","热浸镀锌钢管，φ25*1.2*2400mm","支",14]
[7,"遮阳网","70%遮阳率圆丝遮阳网","m2",3100]
[8,"中间顶柱","热浸镀锌钢管，φ25*1.2*3300mm，垫砖\t","支",88]
[9,"伞骨斜撑","热镀锌钢管φ25*1.2mm,1米一根,一套4根"," 套",88]
[10,"压顶簧","强力钢丝，φ25*25","只",3535]
[11,"外棚门","热浸镀锌钢管，平开门，2m*2m","橙",7]
[12,"U 型卡","热浸镀锌钢管，φ25","付",56]
[13,"外棚卡槽","高锌钢板，0. 7mm","米",1568]
[14,"外棚卡簧","强力钢丝","米",1568]
[15,"卡槽连接片","高锌钢板","只",262]
[16,"外棚抱箍","高铸钢板，φ25","只",56]
[17,"拉杆护套","塑料，φ25","只",42]
[18,"地锚","间距2米","只",707]
[19,"压膜线","300ml卷","米",1590.75]
[20,"外棚卷膜杆","热浸镀锌钢管，φ22*1.2*6000mm","支",117]
[21,"外棚卷膜器","铁质，蓝色加强卷膜器","套",14]
[22,"外棚压膜卡","塑料，φ22","只",1167]
[23,"外棚五金件","高锌材质","批",7]
[24,"外棚顶薄膜","薄膜厚度≥ 0.120mm 长寿防滴膜，12m 宽","㎡",4838.4]
[25,"外棚裙膜","薄膜厚度≥ 0.120mm 长寿防滴膜，0. 6m","㎡",350]
[26,"内部地面处理","素土夯实后铺设黑色园艺地布","㎡",2130]
[27,"安装费",null,"m2",2130]
["连栋温室灌溉清单"]
["序号","材料名称","型号","单位","数量"]
[1,"水泵","QD12-36-1.8KW","台",1]
[2,"逆止阀","DE63","个",1]
[3,"阀门","DE63","个",1]
[4,"过滤器","DE63","个",2]
[5,"PVC管","DE63*0.63MPA","米",100]
[6,"PVC管","DE25*1.6MPA","米",100]
[7,"PE管","LDDE25","米",960]
[8,"倒挂微喷","五件套","套",384]
[9,"主管管道开挖回填","30cm深","米",100]
[10,"排气阀",null,"个",3]
[11,"配件",null,"项",1]
["单体钢架大棚灌溉清单"]
["序号","材料名称","型号","单位","数量"]
[1,"水泵","QD12-36-1.8KW","台",1]
[2,"逆止阀","DE63","个",1]
[3,"阀门","DE63","个",1]
[4,"过滤器","DE63","个",2]
[5,"PVC管","DE63*0.63MPA","米",100]
[6,"PVC管","DE25*1.6MPA","米",70]
[7,"PE管","LDDE25","米",700]
[8,"倒挂微喷","五件套","套",280]
[9,"主管管道开挖回填","30cm深","米",100]
[10,"排气阀",null,"个",3]
[11,"配件",null,"项",1]
["连栋温室苗床清单"]
["序号","材料名称","型号","单位","数量"]
[1,"基础","苗床基础：每组苗床下设计300*300*300mm,C20混凝土基础用于固定苗床基础\n每跨配置苗床规格为宽1.8M×高0.75M，每跨3台，温室内均匀布置。\n２)主要技术参数\n（１）苗床高度：0.75m（地坪至苗床铝合金框上沿）\n（２）苗床宽度：1.8m(苗床铝合金框上沿外边至外边)\n（３）苗床长度： 沿屋脊方向，根据温室建设长度。\n（４）苗床最大承载：25kg/㎡\n３)主要材料规格型号：\n（１）床架立柱□30×30×2㎜\n（２）床架横档□30×20×2㎜（0.5间距）\n（３）床架角撑角钢30×3㎜\n（4）底座钢板3㎜\n（5）网格尺寸（PP塑料）\n（6）铝合金边框 铝型材6061  t2","平方米",1142]
[2,"配件",null,"项",1]
["单体钢架大棚苗床清单"]
["序号","材料名称","型号","单位","数量"]
[1,"基础","苗床基础：每组苗床下设计300*300*300mm,C20混凝土基础用于固定苗床基础\n每跨配置苗床规格为宽1.35M×高0.5M，每跨3台，温室内均匀布置。\n２)主要技术参数\n（１）苗床高度：0.5m（地坪至苗床铝合金框上沿）\n（２）苗床宽度：1.8m(苗床铝合金框上沿外边至外边)\n（３）苗床长度： 沿屋脊方向，根据温室建设长度。\n（４）苗床最大承载：25kg/㎡\n３)主要材料规格型号：\n（１）床架立柱□30×30×2㎜\n（２）床架横档□30×20×2㎜（0.5间距）\n（３）床架角撑角钢30×3㎜\n（4）底座钢板3㎜\n（5）网格尺寸（PP塑料）\n（6）铝合金边框 铝型材6061  t2","平方米",1050]
[2,"配件",null,"项",1]
["温室智能物联网清单"]
["序号","名称","规格","单位","数量"]
[1,"气象站","温度、湿度、光照、雨雪、风向、风速","台",1]
[2,"室内三要素","环境温湿度、光照","台",3]
[3,"LED屏","LED10，960mm*480mm","台",3]
[4,"球机","具有400万像素 ","台",1]
[5,"枪机","具有400万像素 ","台",6]
[6,"核心交换机","型号：RG-NBS5100-24GT4SFP、三层网管交换机，交换容量336Gbps，包转发率51Mpps，24口10/100/1000Mbps自适应电口交换机，固化4个SFP千兆光口，支持静态路由、三层聚合口、ACL、端口镜像等功能，支持睿易APP和MACC云平台统一管理。"," 个",1]
[7,"POE交换","型号：RG-ES205GC-P、4个10/100/1000Mbps电口（支持PoE/PoE+），1个10/100/1000Mbps电口。支持EWEB/APP/MACC管理。","个",2]
[8,"网线","CaT.5E室外防水","箱",1]
[9,"电源线","RVV2*1.5 含穿线管","米",500]
[10,"辅材","立杆、支架、接头、五金等监控必须材料","项",1]
[11,"数据控制软件",null,"套",1]
[12,"云平台租赁",null,"年",3]
["备注“以上材料为全新，报价包含运输、安装、税金"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}