{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"merged":[[0,0,3,4],[5,0,8,0],[5,1,8,1],[5,2,8,2],[5,3,6,3],[5,4,8,4],[7,3,8,3]],"flags":["formulas_cached_only"]}
["采购需求"]
[]
[]
[]
["工程名称：霍山县佛子岭镇卫生院整体迁建项目综合楼外挂污物电梯"]
["序号","项目编码","项目名称","计量","工程量"]
[]
[{"$nulls":3},"单位"]
[]
["1","010101004001","挖基坑土方1.土壤类别：详见图纸及地质勘查资料\r\n2、具体参见施工现场\r\n","m3",30.25]
["2","010103001001","回填方1.密实度要求：压实系数不小于0.94\r\n2.填方材料品种：不应采用建筑垃圾、耕土、腐殖土、淤泥、膨胀土、杂质土等\r\n3.填方粒径要求：符合图纸及相关规范\r\n4.未尽事宜详见图纸及相关规范","m3",21.09]
["3","WB010101013001","余土内运1.土壤类别：详见图纸及地质勘查资料\r\n2.运距：1km\r\n3.含弃土费用、投标人员自行报价，中标后不得更改\r\n","m3",9.16]
["4","WB010101011001","人工清底1.土壤类别：详见图纸及地质勘查资料\r\n2.清底厚度：满足设计及规范要求\r\n","m2",8.526]
["5","010404001001","C15砼基础垫层（P6)1.厚度：100厚\r\n2.材料品种及比例：C15砼（P6)\r\n3.部位：垫层","m3",0.853]
["6","011702001001","C15砼基础垫层模板1、基础类型：基础垫层\r\n2、材质：木质\r\n","m2",1.168]
["7","010501004001","C30电梯基础（P6)1、混凝土种类：商品砼\r\n2、混凝土强度等级：C30(P6)\r\n3、具体做法参见图纸设计","m3",2.959]
["8","011702001001","C30电梯基础模板1、基础类型：电梯基础\r\n2、材质：木质","m2",4.352]
["9","010504001001","C30电梯井壁（P6)1、混凝土种类：商品砼\r\n2、混凝土强度等级：C30(P6)\r\n3、厚度：250mm\r\n4、具体做法参见图纸设计","m3",2.924]
["10","011702011001","C30电梯井壁模板1.类型：电梯井壁模板\r\n2、材质：木质","m2",23.392]
["11","010515001002","现浇构件钢筋1.现浇构件钢筋","t",0.345]
["12","011702011001","电梯电梯购安暂定180000元/套，含安装和所有配件，具体价格以决算时所发生价格为准。\r\n","套",1]
["13","011705001001","大型机械设备进出场及安拆1、大型机械设备进出场及安拆\r\n2、具体参见设计图纸及相关规范和法律法规","台次",1]
[null,null,"合    计"]
["安徽省建设工程造价计价软件测评合格编号2018JS-02"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}