{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["2 E.1 分部分项工程量清单计价表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"2 E.1 分部分项工程量清单计价表","index":0,"n_rows":160,"n_cols":8,"rows_kept":160,"merged":[[0,0,0,7],[1,0,1,3],[1,4,1,5],[1,6,1,7],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,2,7],[4,2,4,3],[29,2,29,3],[38,2,38,3],[53,2,53,3],[60,2,60,3],[68,2,68,3],[76,2,76,3],[83,2,83,3],[85,2,85,3],[94,2,94,3],[100,2,100,3],[107,2,107,3],[121,2,121,3],[132,2,132,3],[142,2,142,3],[148,2,148,3],[159,3,159,7]],"flags":["formulas_cached_only"]}
["E.1 分部分项工程量清单计价表",null,null,"","","","",""]
["工程名称：2025年霍山县乡源供水有限公司维修改造劳务采购项目",null,null,"","","","",""]
["序号","项目编码","项目名称","项目特征描述","计量\n单位","工程量","金额（元）",""]
[{"$nulls":3},"","","","综合单价","合价"]
[null,"一","土石方开挖及回填","","","","",1917.36]
["1","040101002001","挖沟槽土方（试用管径20-40）","1.挖、填沟槽土方（试用管径20-40）\n2.土壤类别：土或土石混合料\n3.开挖方式：自定\n4.规格：20*40cm","m",1,5.48,5.48]
["2","040101002002","挖沟槽土方（试用管径50-63）","1.挖、填沟槽土方（试用管径50-63）\n2.土壤类别：土或土石混合料\n3.开挖方式：自定\n4.规格：40*35cm","m",1,10.31,10.31]
["3","040101002003","挖沟槽土方（试用管径75-100）","1.挖、填沟槽土方（试用管径75-100）\n2.土壤类别：土或土石混合料\n3.开挖方式：自定\n4.规格：50*40cm","m",1,16.72,16.72]
["4","040101002004","挖沟槽土方（试用管径150-200）","1.挖、填沟槽土方（试用管径150-200）\n2.土壤类别：土或土石混合料\n3.开挖方式：自定\n4.规格：60*40cm","m",1,16.83,16.83]
["5","040101002005","挖沟槽土方（试用管径250-300）","1.挖、填沟槽土方（试用管径250-300）\n2.土壤类别：土或土石混合料\n3.开挖方式：自定                                \n 4.规格：70*50cm","m",1,19.91,19.91]
["6","040101002006","挖沟槽土方（试用管径400）","1.挖、填沟槽土方（试用管径400）\n2.土壤类别：土或土石混合料\n3.开挖方式：自定                               \n4.规格：70*50cm","m",1,25.02,25.02]
["7","040102001001","挖一般石方","1.挖一般石方（挖一般石方、回填）         \n2.工作内容：石方开挖                            \n3.含石方外运，运距自定，中标后不给予调整 \n4.含渣土费\n5.清单项目特征不完善处,依据规范,满足使用功能","m3",1,182.61,182.61]
["8","011705001003","大型机械设备进出场及安拆","1.大型机械设备进出场及安拆\n2.160以下挖机\n3.用于抢修（一天以内），机械调运费，一天以外无此项费用","台次",1,500,500]
["9","041001001001","拆除沥青路面（拆除厚度：10cm）","1.沥青路面拆除 （拆除厚度：10cm）                                                                                                 2.清单项目特征不完善处,依据规范,满足使用功能","m2",1,14.38,14.38]
["10","041001001004","拆除混凝土路面（拆除厚度：10cm）","1.机械拆除混凝土路面（拆除厚度：10cm）\n2.清单项目特征不完善处,依据规范,满足使用功能","m2",1,7.07,7.07]
["11","041001001003","拆除混凝土路面（拆除厚度：15cm）","1.机械拆除混凝土路面（拆除厚度：15cm）\n2.清单项目特征不完善处,依据规范,满足使用功能","m2",1,11.52,11.52]
["12","041001001002","拆除混凝土路面（拆除厚度：20cm）","1.机械拆除混凝土路面（拆除厚度：20cm）\n2.清单项目特征不完善处,依据规范,满足使用功能","m2",1,15.95,15.95]
["13","041001008001","拆除混凝土结构","1.拆除混凝土结构\n2.拆除方式：自定\n3.清单项目特征不完善处,依据规范,满足使用功能","m3",1,268.6,268.6]
["14","WB011614004001","建筑垃圾外运","1.建筑垃圾外运\n2.运距自定，中标后不给予调整\n3.渣土费2元/m3","m3",1,28.53,28.53]
["15","040202001002","20cm厚C30水泥混凝土基层(沥青路面基层，含主材）","1.20cm厚C30水泥混凝土路面(商品砼，含主材）水泥混凝土路面                        \n2.混凝土等级：C30商品混凝土                     \n3.工作内容：路床(槽)碾压检验，铺设路面、模板                  \n4.清单项目特征不完善处,依据规范,满足使用功能","m2",1,119.43,119.43]
["16","040203006001","沥青混凝土面层（6cm+4cm）","1.沥青混凝土面层（6c+4cm）6cmAC20粗粒式沥青+4cmAC13C改性细粒是沥青\n2.工作内容：透层、粗粒式沥青混凝土面层~厚6cm，粘层、细粒式沥青混凝土路面~厚4cm，封层\n3.清单项目特征不完善处,依据规范,满足使用功能","m2",1,145.52,145.52]
["17","040203007002","C30水泥混凝土路面修补","1.C30水泥混凝土路面(商品砼，含主材）路面厚度不小于10cm\n2.混凝土等级：C30商品混凝土\n3.工作内容：路床(槽)碾压检验，铺设路面、模板、养护、刻痕\n4.清单项目特征不完善处,依据规范,满足使用功能","m2",1,95.82,95.82]
["18","050101010001","铺种马尼拉草皮（含主材）","1.铺种马尼拉草皮（含主材）铺种草皮\n2.工作内容：铺种草皮，草坪成活养护，草坪保存养护\n3.二级养护\n4.养护时间：含1个月成活养护，11个月保存养护","m2",1,41.4,41.4]
["19","041001007001","人行道、广场砖拆除","1.方块砖拆除（含基层拆除，垃圾外运）方块砖拆除\n2.清单项目特征不完善处,依据规范,满足使用功能","m2",1,9.24,9.24]
["20","010401003003","人行道、广场砖铺装","1.人行道、广场砖铺装\n2.2cm厚水泥砂浆垫层\n3.清单项目特征不完善处,依据规范,满足使用功能","m2",1,53.76,53.76]
["21","040204003001","8cm人行道混凝土垫层恢复（商品砼）","1.8cm人行道混凝土垫层恢复（商品砼，含主材）1.8cm人行道混凝土垫层\n2.混凝土类型：C20商品混凝土\n3.工作内容：8cm人行道混凝土垫层、模板\n4.清单项目特征不完善处,依据规范,满足使用功能","m2",1,56.03,56.03]
["22","040204003002","8cm人行道混凝土垫层恢复（自拌砼）","1.8cm人行道混凝土垫层恢复（自拌砼，含主材）1.8cm人行道混凝土垫层\n2.混凝土类型：C20商品混凝土\n3.工作内容：8cm人行道混凝土垫层、模板\n4.清单项目特征不完善处,依据规范,满足使用功能","m2",1,50.61,50.61]
["23","041001007003","水表井拆除","1.水表井拆除\n2.规格：不小于300*500mm\n3.含垃圾外运，运距自定，中标后不给予调整","座",1,13.4,13.4]
["24","040601010001","20cm厚C25现浇混凝土盖板","1.C25现浇混凝土盖板\n2.厚度：20cm\n2.钢筋规格：φ25@150单层双向","m2",1,209.22,209.22]
[null,"二","井体砌筑","","","","",4860.92]
["25","WB040504016001","小型井（300*500）","1.小型井（300*500）\n2.工作内容：含挖、填土方，余方就近弃置，内外抹灰\n3.壁厚：12cm，井深40cm\n4、甲供铸铁井盖或复合井盖，含材料运费、安装\n5.清单项目特征不完善处,依据规范,满足使用功能","座",1,201.07,201.07]
["26","WB040504016002","中型井（500*500）","1.小型井（500*500）\n2.工作内容：含挖、填土方，余方就近弃置，内外抹灰\n3.壁厚：12cm，井深40cm\n4、甲供铸铁井盖或复合井盖，含材料运费、安装含材料运费、安装\n5.清单项目特征不完善处,依据规范,满足使用功能","座",1,223.18,223.18]
["27","WB040504016003","表井组（500*800）","1.表井组（500*800）\n2.工作内容：含挖、填土方，余方就近弃置，内外抹灰\n3.壁厚：12cm，井深40cm\n4、甲供铸铁井盖或复合井盖，含材料运费、安装\n5.清单项目特征不完善处,依据规范,满足使用功能","座",1,256.38,256.38]
["28","WB040504016004","表井组（500*1000）","1.表井组（500*1000）\n2.工作内容：含挖、填土方，余方就近弃置，内外抹灰\n3.壁厚：12cm，井深40cm\n4、甲供铸铁井盖或复合井盖，含材料运费、安装含材料运费、安装\n5.清单项目特征不完善处,依据规范,满足使用功能","座",1,278.47,278.47]
["29","WB040504016005","圆形井","1.圆形井\n2.工作内容：外径1.1m，高1m，含挖、填土方，余方就近弃置，内外抹灰\n3.壁厚：24cm，井深100cm\n4.25cm厚·C25预制钢筋混凝土盖板,φ25@150,单层双向（包含预制井盖），含材料运费、安装\n5.清单项目特征不完善处,依据规范,满足使用功能","座",1,1017.46,1017.46]
["30","WB040504015001","闸阀井（1*1*1米，井盖甲供）","1.闸阀井（1*1*1米，井盖甲供）DN100闸阀井（1*1*1米）                         \n 2.清单项目特征不完善处,依据规范,满足使用功能","座",1,780.39,780.39]
["31","WB040504015002","闸阀井（1.2*1.2*1米，井盖甲供）","1.N150-200闸阀井（1.2*1.2*1米，井盖甲供）DN150-200闸阀井（1.2*1.2*1米）                                                            2.清单项目特征不完善处,依据规范,满足使用功能","座",1,980.09,980.09]
["32","WB040504015003","闸阀井（1.4*1.2*1米，井盖甲供）","1、闸阀井（1.4*1.2*1米，井盖甲供）                                                    2、清单项目特征不完善处,依据规范,满足使用功能","座",1,1123.88,1123.88]
[null,"三","其他零星工程","","","","",2469.39]
["33","010404001001","填砂","1.填砂\n2.清单项目特征不完善处,依据规范,满足使用功能","m3",1,287.9,287.9]
["34","010404001003","填石粉","1.填石粉\n2.清单项目特征不完善处,依据规范,满足使用功能","m3",1,247.86,247.86]
["35","010404001004","填混合砂","1.填混合砂\n2.清单项目特征不完善处,依据规范,满足使用功能","m3",1,308.72,308.72]
["36","010401003001","120实心砖墙（含主材）","1.120实心砖墙\n2.清单项目特征不完善处,依据规范,满足使用功能","m2",1,72.03,72.03]
["37","010401003002","240实心砖墙（含主材）","1.240实心砖墙\n2.清单项目特征不完善处,依据规范,满足使用功能","m2",1,142.91,142.91]
["38","011201001001","墙面一般抹灰","1.墙面一般抹灰\n2.厚度：20mm\n3. 1∶2.5水泥砂浆、1∶3水泥砂浆","m2",1,36.3,36.3]
["39","011615001001","开墙洞（直径6cm）","1.开墙洞（直径6cm）\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,34.24,34.24]
["40","011615001002","开墙洞（直径12cm）","1.开墙洞（直径12cm）\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,57.99,57.99]
["41","WB041111005001","浆砌石挡墙","1.浆砌石挡墙\n2.清单项目特征不完善处,依据规范,满足使用功能","m3",1,509.98,509.98]
["42","011705001001","挖机","1.挖机\n2.清单项目特征不完善处,依据规范,满足使用功能","台时",1,231.66,231.66]
["43","011705001002","吊机","1.吊机\n2.清单项目特征不完善处,依据规范,满足使用功能","台时",1,211.83,211.83]
["44","ZB040101001003","人工","1.人工\n2.工种自定\n3.清单项目特征不完善处,依据规范,满足使用功能","工日",1,230.03,230.03]
["45","030901011001","DN80-100室外消防栓安装（不含主材）","1.地上式室外消防栓（含消火栓、三通安装）\n2.公称直径：DN80-100\n3.清单项目特征不完善处,依据规范,满足使用功能","套",1,90,90]
["46","WB031002006002","预留管洞（支模清扫）","1.预留管洞（支模清扫）\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,7.94,7.94]
[null,"四","室外铸铁给水铸铁管（胶圈接口）","","","","",99.21]
["47","030801019002","铸铁给水管DN100（不含主材）","1.名称:铸铁给水管，不含主材\n2.介质:给水管\n3.工地现场吊运，检查及清扫管材、切管、组对、管道及管件安装、安装胶圈\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,7.12,7.12]
["48","030801019003","铸铁给水管DN150（不含主材）","1.名称:铸铁给水管，不含主材\n2.介质:给水管\n3.工地现场吊运，检查及清扫管材、切管、组对、管道及管件安装、安装胶圈\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,9.36,9.36]
["49","030801019004","铸铁给水管DN200（不含主材）","1.名称:铸铁给水管，不含主材\n2.介质:给水管\n3.工地现场吊运，检查及清扫管材、切管、组对、管道及管件安装、安装胶圈\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,14.12,14.12]
["50","030801019005","铸铁给水管DN250（不含主材）","1.名称:铸铁给水管，不含主材\n2.介质:给水管\n3.工地现场吊运，检查及清扫管材、切管、组对、管道及管件安装、安装胶圈\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,16.35,16.35]
["51","030801019006","铸铁给水管DN300（不含主材）","1.名称:铸铁给水管，不含主材\n2.介质:给水管\n3.工地现场吊运，检查及清扫管材、切管、组对、管道及管件安装、安装胶圈\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,23.32,23.32]
["52","030801019007","铸铁给水管DN400（不含主材）","1.名称:铸铁给水管，不含主材\n2.介质:给水管\n3.工地现场吊运，检查及清扫管材、切管、组对、管道及管件安装、安装胶圈\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,28.94,28.94]
[null,"五","新安装室外塑料给水管（热熔连接）安装","","","","",172.07]
["53","031001006016","塑料给水管DN15-32（不含主材）","1.名称:塑料给水管，不含主材\n2.介质:给水管\n3.切管、坡口加工、管口组对、管件熔接、管道及管件安装、水压试验及水冲洗\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,4.56,4.56]
["54","031001006005","塑料给水管DN40-63（不含主材）","1.名称:塑料给水管，不含主材\n2.介质:给水管\n3.切管、坡口加工、管口组对、管件熔接、管道及管件安装、水压试验及水冲洗\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,5.03,5.03]
["55","031001006006","塑料给水管DN75-110（不含主材）","1.名称:塑料给水管，不含主材\n2.介质:给水管\n3.切管、坡口加工、管口组对、管件熔接、管道及管件安装、水压试验及水冲洗\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,6.25,6.25]
["56","031001006007","塑料给水管DN125-160（不含主材）","1.名称:塑料给水管，不含主材\n2.介质:给水管\n3.切管、坡口加工、管口组对、管件熔接、管道及管件安装、水压试验及水冲洗\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,13.4,13.4]
["57","040501004001","塑料给水管DN200-250（不含主材）","1.名称:塑料给水管，不含主材\n2.介质:给水管\n3.切管、坡口加工、管口组对、管件熔接、管道及管件安装、水压试验及水冲洗\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,34.22,34.22]
["58","040501004002","塑料给水管DN300-500（不含主材）","1.名称:塑料给水管，不含主材\n2.介质:给水管\n3.切管、坡口加工、管口组对、管件熔接、管道及管件安装、水压试验及水冲洗\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,100.85,100.85]
["59","031001007001","钢丝给水管DN75-160（不含主材）","1.名称:钢丝给水管，不含主材\n2.介质:给水管\n3.切管、坡口加工、管口组对、管件熔接、管道及管件安装、水压试验及水冲洗\n4.清单项目特征不完善处,依据规范,满足使用功能","m",1,7.76,7.76]
[null,"六","阀门（螺纹式、法兰式含止回阀）安装","","","","",433.75]
["60","031003001001","螺纹阀门DN15-20（不含主材）","1..类型:螺纹阀门（不含主材）\n2.阀门检查及研磨、阀门安装、垂直运输、阀门调试\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,8.67,8.67]
["61","031003001002","螺纹阀门DN25-32（不含主材）","1..类型:螺纹阀门（不含主材）\n2.阀门检查及研磨、阀门安装、垂直运输、阀门调试\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,11.03,11.03]
["62","031003001003","螺纹阀门DN40-63（不含主材）","1..类型:螺纹阀门（不含主材）\n2.阀门检查及研磨、阀门安装、垂直运输、阀门调试\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,21.05,21.05]
["63","031003003001","焊接法兰阀门DN80-100（不含主材）","1.类型:焊接法兰阀门含止回阀（不含主材）\n2.阀门检查及研磨、阀门安装、垂直运输、阀门调试\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,40.23,40.23]
["64","031003003002","焊接法兰阀门DN150-200（不含主材）","1.类型:焊接法兰阀门含止回阀（不含主材）\n2.阀门检查及研磨、阀门安装、垂直运输、阀门调试\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,75.16,75.16]
["65","031003003003","焊接法兰阀门DN250-300（不含主材）","1.类型:焊接法兰阀门含止回阀（不含主材）\n2.阀门检查及研磨、阀门安装、垂直运输、阀门调试\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,107.25,107.25]
["66","031003003004","焊接法兰阀门DN350-400（不含主材）","1.类型:焊接法兰阀门含止回阀（不含主材）\n2.阀门检查及研磨、阀门安装、垂直运输、阀门调试\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,170.36,170.36]
[null,"七","水表（螺纹式、法兰式含过滤器）安装","","","","",124.45]
["67","031003013001","螺纹式水表DN15-25（不计主材）","1.类型:螺纹式水表，不计主材（接水入户新安装水表）\n2.清洗检查，对接安装，上螺栓\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,5.28,5.28]
["68","031003013006","螺纹式水表DN15-25（不计主材）","1.类型:螺纹式水表，不计主材（维修抢修更换水表）\n2.清洗检查，对接安装，上螺栓\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,27.54,27.54]
["69","031003013002","螺纹式水表DN40（不计主材）","1.类型:螺纹式水表，不计主材\n2.清洗检查，对接安装，上螺栓\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,7,7]
["70","031003013003","法兰式水表DN50（不计主材）","1.类型:法兰式含过滤器，不计主材\n2.清洗检查，对接安装，上螺栓\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,14.13,14.13]
["71","031003013004","法兰式水表DN80-100（不计主材）","1.类型:法兰式含过滤器，不计主材\n2.清洗检查，对接安装，上螺栓\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,28.25,28.25]
["72","031003013005","法兰式水表DN150-200（不计主材）","1.类型:法兰式含过滤器，不计主材\n2.清洗检查，对接安装，上螺栓\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,42.25,42.25]
[null,"八","远传水表（不计主材）","","","","",60.91]
["73","WB031002003001","入地表箱安装（不计主材）","1.名称:入地表箱安装（不计主材）\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,60.91,60.91]
[null,"九","法兰片安装","","","","",270.27]
["74","031003011001","法兰片安装DN50（不含主材）","1.名称:不锈钢平焊法兰片安装，不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","副",1,8.25,8.25]
["75","031003011002","法兰片安装DN80（不含主材）","1.名称:不锈钢平焊法兰片安装，不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","副",1,11,11]
["76","031003011003","法兰片安装DN100（不含主材）","1.名称:不锈钢平焊法兰片安装，不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","副",1,14,14]
["77","031003011004","法兰片安装DN150（不含主材）","1.名称:不锈钢平焊法兰片安装，不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","副",1,20.63,20.63]
["78","031003011005","法兰片安装DN200（不含主材）","1.名称:不锈钢平焊法兰片安装，不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","副",1,27.88,27.88]
["79","031003011006","法兰片安装DN250（不含主材）","1.名称:不锈钢平焊法兰片安装，不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","副",1,43.13,43.13]
["80","031003011007","法兰片安装DN300（不含主材）","1.名称:不锈钢平焊法兰片安装，不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","副",1,61.88,61.88]
["81","031003011009","法兰片安装DN400（不含主材）","1.名称:不锈钢平焊法兰片安装，不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","副",1,83.5,83.5]
[null,"十","分户器安装","","","","",79.03]
["82","031003004001","分户器安装（二组）（不含主材）","1.名称:分户器安装（二组），不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,6.81,6.81]
["83","031003004002","分户器安装（三组）（不含主材）","1.名称:分户器安装（三组），不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,10.9,10.9]
["84","031003004003","分户器安装（四组）（不含主材）","1.名称:分户器安装（四组），不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,16.35,16.35]
["85","031003004004","分户器安装（五组）（不含主材）","1.名称:分户器安装（五组），不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,20.44,20.44]
["86","031003004005","分户器安装（六组）（不含主材）","1.名称:分户器安装（六组），不含主材\n2.配组检查，螺栓连接，对接安装\n3.清单项目特征不完善处,依据规范,满足使用功能","组",1,24.53,24.53]
[null,"十一","管道运费","","","","",30.82]
["87","ZB030101001001","塑料给水管DN20-32（管道运费）","1.名称:管道运费\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,0.33,0.33]
["88","ZB030101001002","塑料给水管DN40-63（管道运费）","1.名称:管道运费\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,0.83,0.83]
["89","ZB030101001003","塑料给水管DN75-160（管道运费）","1.名称:管道运费\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,1.31,1.31]
["90","ZB030101001004","塑料给水管DN200-300（管道运费）","1.名称:管道运费\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,1.65,1.65]
["91","ZB030101001005","球墨铸铁给水管DN200-300（管道运费）","1.名称:管道运费\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,9.9,9.9]
["92","ZB030101001006","球墨铸铁给水管DN400-600（管道运费）","1.名称:管道运费\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,16.8,16.8]
[null,"十二","室外钢管（焊接），不计主材","","","","",1720.83]
["93","031001002001","室外钢管DN50(焊接）（不计主材）","1.名称:室外钢管DN50(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,14.07,14.07]
["94","031001002002","室外钢管DN65(焊接）（不计主材）","1.名称:室外钢管DN65(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,17.43,17.43]
["95","031001002003","室外钢管DN80(焊接）（不计主材）","1.名称:室外钢管DN80(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,20.57,20.57]
["96","031001002004","室外钢管DN100(焊接）（不计主材）","1.名称:室外钢管DN100(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,33.19,33.19]
["97","031001002005","室外钢管DN150(焊接）（不计主材）","1.名称:室外钢管DN150(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,45.34,45.34]
["98","031001002006","室外钢管DN200(焊接）（不计主材）","1.名称:室外钢管DN200(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,58.87,58.87]
["99","031001002007","室外钢管DN300(焊接）\n（不计主材）","1.名称:室外钢管DN300(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,99.12,99.12]
["100","031001002008","室外钢管DN400(焊接）（不计主材）","1.名称:室外钢管DN400(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,128.6,128.6]
["101","031001002009","室外钢管DN500(焊接）（不计主材）","1.名称:室外钢管DN500(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,169.62,169.62]
["102","030801007001","室外钢管DN600(焊接）（不计主材）","1.名称:室外钢管DN600(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,182.97,182.97]
["103","030801007002","室外钢管DN800(焊接）（不计主材）","1.名称:室外钢管DN800(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,245.62,245.62]
["104","030801007003","室外钢管DN1000(焊接）（不计主材）","1.名称:室外钢管DN1000(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,317.95,317.95]
["105","030801007004","室外钢管DN1200(焊接）（不计主材）","1.名称:室外钢管DN1200(焊接）\n2.清单项目特征不完善处,依据规范,满足使用功能","m",1,387.48,387.48]
[null,"十三","室外管道抱箍安装","","","","",3252.05]
["106","031002003001","DN100抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,52.32,52.32]
["107","031002003003","DN150抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,70.85,70.85]
["108","031002003004","DN200抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,94.83,94.83]
["109","031002003005","DN300抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,144.97,144.97]
["110","031002003006","DN400抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,221.27,221.27]
["111","031002003007","DN500抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,279.04,279.04]
["112","031002003008","DN600抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,394.07,394.07]
["113","031002003009","DN800抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,513.39,513.39]
["114","031002003010","DN1000抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,668.17,668.17]
["115","031002003011","DN1200抱箍安装","1.破损管道修复\n2.抱箍焊接\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,813.14,813.14]
[null,"十四","室外钢管，管件制作，挖眼三通，不含主材","","","","",2838.66]
["116","WB030814003001","DN100钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,109.76,109.76]
["117","WB030814003004","DN150钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,134.83,134.83]
["118","WB030814003002","DN200钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,181.7,181.7]
["119","WB030814003005","DN300钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,235.11,235.11]
["120","WB030814003006","DN400钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,287.43,287.43]
["121","WB030814003007","DN500钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,346.29,346.29]
["122","WB030814003008","DN600钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,388.8,388.8]
["123","WB030814003009","DN800钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,527.23,527.23]
["124","WB030814003010","DN1000钢管挖眼，焊接管件","1.钢管挖眼，焊接管件\n2.清单项目特征不完善处,依据规范,满足使用功能","个",1,627.51,627.51]
[null,"十五","其他","","","","",441.95]
["125","WB031002005001","PE给水管DN50及以下开三通","1.名称:DN50及以下开孔\n2.维修PE管开口、改造\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,45.78,45.78]
["126","WB031002005002","PE给水管DN50-100开三通","1.名称:DN50-100开孔\n2.维修PE管开口、改造\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,61.04,61.04]
["127","WB031002005003","PE给水管DN100开三通","1.名称:DN100开孔\n2.维修PE管开口、改造\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,114.45,114.45]
["128","ZB030101001007","PE给水管DN160开三通","1.名称:DN160开孔\n2.维修PE管开口、改造\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,183.12,183.12]
["129","031002001001","50*5镀锌角钢支架（含主材）","1.50*5镀锌角钢支架\n2.制作安装\n3.清单项目特征不完善处,依据规范,满足使用功能","个",1,37.56,37.56]
[null,"十六","零星供水维修","","","","",1304.8]
["130","031001006017","PE给水管维修DN20-DN25管（不计主材、不含土方开挖）","1.不含土方开挖\n2.除清单特征外以上条件满足其中一项均以零星供水维修计算作为结算依据","处",1,30,30]
["131","031001006008","PE给水管维修DN20-DN25管（不计主材）","1.管道开挖长度5m以内 \n2.土方开挖方量1.5m3以内                                 3.混凝土开挖方量在1m3以内                                                       4.除清单特征外以上条件满足其中一项均以零星供水维修计算作为结算依据","处",1,58,58]
["132","031001006009","PE给水管维修DN32-DN50管（不计主材）","1.管道开挖长度5m以内 \n2.土方开挖方量1.5m3以内                                 3.混凝土开挖方量在1m3以内                                                       4.除清单特征外以上条件满足其中一项均以零星供水维修计算作为结算依据","处",1,76,76]
["133","031001006010","PE给水管维修DN63-DN75管（不计主材）","1.管道开挖长度5m以内 \n2.土方开挖方量1.5m3以内                                 3.混凝土开挖方量在1m3以内                                                       4.除清单特征外以上条件满足其中一项均以零星供水维修计算作为结算依据","处",1,158,158]
["134","031001006011","PE给水管维修DN90-DN110管（不计主材）","1.管道开挖长度5m以内 \n2.土方开挖方量1.5m3以内                                 3.混凝土开挖方量在1m3以内                                                       4.除清单特征外以上条件满足其中一项均以零星供水维修计算作为结算依据","处",1,200,200]
["135","031001006012","PE给水管哈夫节维修DN75-110管（不计主材）","1.管道开挖长度5m以内 \n2.土方开挖方量1.5m3以内                                 3.混凝土开挖方量在1m3以内                 \n4.哈夫节维修需经发包单位审核后，确定是否使用","处",1,120,120]
["136","031001006013","PE给水管哈夫节维修DN150-200管（不计主材）","1.管道开挖长度5m以内 \n2.土方开挖方量1.5m3以内                                 3.混凝土开挖方量在1m3以内                 \n4.哈夫节维修需经发包单位审核后，确定是否使用","处",1,240,240]
["137","031001006014","PE给水管哈夫节安装250-300管（不计主材）","1.管道增接口\n2.哈夫节安装需经发包单位审核后，确定是否可行","处",1,200,200]
["138","031001006015","PE给水管哈夫节安装355-400管（不计主材）","1.管道增接口\n2.哈夫节安装需经发包单位审核后，确定是否可行","处",1,220,220]
["139","ZB030101001008","冬季保暖措施安装","1.冬季保暖措施安装","个",1,2.8,2.8]
[{"$nulls":3},"","","","",""]